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MX-5050 SERIES PROFESSIONAL RECORDER — INTRODUCTION
This manual supplement provides detailed maintenance information, schematics, and parts lists for the Otari MX-5050 Series Models 2S, 4S, 2SD and 4SD Professional Recorder. For descriptive information, installation and operating instructions, preventive maintenance and routine adjustment procedures, refer to Otari Instruction Manual Catalog No. OIM-1005E.
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MX-5050 2SD Recorder


COMMUNICATION WITH OTARI — FOR SERVICE INFORMATION AND PARTS
The OTARI PRODUCTS are manufactured under strict quality control and each unit was carefully tested and inspected prior to shipment from our factory.
If, however, some adjustments or technical support become necessary, replacement parts are required, or technical questions arise, please contact your nearest Otari dealer or write to:
	OTARI ELECTRIC CO., LTD.
	OTARI CORPORATION

	4-29-18, Minami Ogikubo,
	1559 Industrial Road, San Carlos,

	Suginamiku, Tokyo, 167, Japan
	California 94070, U. S. A.

	Phone: (03) 333 - 9631
	Phone: (415) 592 - 8311

	Telex No.: OTRDENKI J26604
	Telex No.: TWX 910-376-4890


Another part of Otari continuous technical support program for our products, is the continuous revision of manuals as the equipment is improved or modified.
In order for you to receive our information and service applicable to your requirement, and for the technical support to function properly, please include the following information, most of which can be obtained from the name plate on the equipment.
1. Model Number
1. Serial Number
1. Date of purchase
1. Name and address of dealer from whom machine was purchased.
1. Power requirements (voltage and frequency)
1. Manual number which you are referring
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SECTION 1 — GENERAL INFORMATION
This manual is a maintenance supplement to the MX-5050 Series Models 2S, 4S, 2SD and 4SD Instruction Manual, Catalog No. OIM-1005E, and provides detailed maintenance information. This manual is intended for use by qualified maintenance or service personnel only. Prior to using this manual, it is suggested that the user become familiar with the information contained in the basic manual.
NOTE
AFTER MAINTENANCE OR COMPONENT REPLACEMENT, ALL SCREWS SHOULD BE LOCKED UP WITH FOLLOWING PAINT TO PREVENT POSSIBLE DAMAGE. USE ENAMEL PAINT FOR HEAD ALIGNMENT SCREWS (AZIMUTH, ZENITH, HEIGHT), AND USE LOCTITE-222 (VIOLET) FOR OTHER SCREWS.
1-1 TEST AND MAINTENANCE EQUIPMENT REQUIREMENTS
All maintenance, electronic, and mechanical test equipment required during maintenance, alignment, and adjustment of the recorder is listed in Table 1-1. In addition, recommended maintenance periods are shown by accumulative hours of usage and/or elapsed period of time, whichever occurs first. Equivalent equipment can be substituted for the equipment suggested in the table.
Table 1-1. Test and Maintenance Equipment
	EQUIPMENT TYPE
	SUGGESTED MODEL
	USED FOR
	PERIOD

	Head cleaner
	Ampex 087-007
	Cleaning heads and guides
	8 hours

	Isopropyl or denatured alcohol
	Any
	Cleaning capstan pinch-roller
	8 hours

	Q tips
	Any
	Cleaning heads and guides
	8 hours

	Head demagnetizer
	Ampex 4010820
	Demagnetizing heads and guides
	8 hours

	Lubricating oil
	Ampex 087-579 or Mobile [sic] DTE Medium
	Oiling of capstan motor and pinch roller bearings
	1,000 hours or 6 months

	Spring scales 0-16 oz, 0-32 oz and 0-10 lbs
	Any
	Mechanical adjustments
	1,000 hours or 6 months

	Frequency Counter (Electronic Counter)
	Hewlett-Packard 5300A + 5301A
	Tape speed measurment [sic]
	Same as above

	Vacuum cleaner and brushes
	Any
	General cleaning
	1 month

	Standard alignment test tapes
	Refer to Table 1-2 and 1-3.
	Reproduce amplifier alignment
	150 hours or 1 month

	Audio oscillator
	Hewlett Packard H20-200CD
	Overall frequency response and signal-to-noise measurement
	150 hours or 1 month

	AC Voltmeter (VTVM)
	Hewlett Packard 400L or 400 FL
	Same as above
	Same as above

	Bandpass filter
	See text
	Same as above
	Same as above

	Flutter bridge
	Data Measurement Corp. 8100
	Flutter and wow measurement
	Same as above

	Wave analyzer
	Hewlett Packard 3590A or 310A
	Distortion and crosstalk measurement
	Same as above

	Test cables
	See text
	
	

	Technicians tools
	
	
	

	Stroboscope
	General Radio 1531-AB
	Mechanical adjustments
	1,000 hours or 6 months

	Volt-ohm meter
	20,000 ohms/volt any brank [sic]
	Test and adjustments
	-

	Allen wrenches
	Metric
	
	

	ASA Noise Filter
	See text and Fig. 3-1.
	Signal-to-noise ratio measurement
	150 hours or 1 month


Table 1-2. Alignment Test Tape
	SPEED (IN/S)
	EQUALIZATION (TIME CONSTANTS)
	STANDARD
	TRACKS
	AMPEX CATALOG NO.

	3-3/4
	90 μs & 3180 μs
	NAB
	Full
	4690037-01

	7-1/2
	50 μs & 3180 μs
	NAB
	Full
	01-31321-01

	
	50 μs & 3180 μs
	NAB
	1 & 3
	01-31321-04

	
	70 μs & ∞
	IEC
	Full
	4690014-01

	15
	50 μs & 3180 μs
	NAB
	Full
	01-31311-01

	
	35 μs & ∞
	IEC
	Full
	01-31313-01


1-2 ROUTINE MAINTENANCE
It is important that routine maintenance be performed at the recommended intervals. External cleaning and demagetization [sic] procedures should be performed after each eight hours of operation, and the interior of the transport should be cleaned once a month. The lubrication procedure should be performed after 1,000 hours of operation or after 6 months, whichever comes first.
1-2-(1) CLEANING
Oxide particles from the magnetic tape tend to collect on components in the tape path and degrade performance of the recorder. To clean the head assembly, proceed as follows:
1. Lift the head cover as shown in Fig. 1-1.
CAUTION
WHEN CLEANING THE HEADS, USE ONLY THE RECOMMENDED SOLVENT (HEAD CLEANER) TO AVOID DAMAGING THE HEADS. KEEP THE HEAD CLEANER OFF PLASTIC FINISHES AND THE CAPSTAN PINCH ROLLER. DO NOT USE METAL TOOLS THAT CAN SCRATCH THE HEADS.
1. Clean each head stack thoroughly with a cotton-tipped applicator (Q tip) dampened with head cleaner.
1. Use isopropyl alcohol to clean all tape-guiding components, the capstan shaft, and the capstan pinch roller.
CAUTION
DO NOT USE HEAD CLEANER ON THE CAPSTAN PINCH ROLLER AS DAMAGE WILL RESULT AND TAPE WILL SLIP.

Fig. 1-1 Lifting Head Cover
1. Remove rear cover of recorder (4 screws).
1. Use a vacuum cleaner and a small brush to remove all dust or contamination from the interior of the transport. If necessary lightly moisten brush with isopropyl alcohol to clean parts.
1. Reinstall rear cover.
1-2-(2) DEMAGNETIZING
The heads and tape guiding components in the tape path should be demagnetized after each eight hours of operation. These components can acquire permanent magnetization that increases signal noise and distortion and partially erase high frequencies on recorded tape. Use a hand-held head demagnetizer to demagnetize all components in the tape path as follows:
1. Turn equipment power off and remove any recorded tape near the transport (tape could be partially erased by the demagnetizer).
1. Lift head cover as shown in Figure 1-1.
1. Cover the demagnetizer tips with adhesive tape to prevent scratching head stacks.
1. With the demagnetizer held away from the transport, connect demagnetizer to power source.
1. Move the demagnetizer tips slowly close to the head, lightly touch the demagnetizer tips to the face of one head stack and slowly move the tips up and down the stack several times. Then slowly withdraw the demagnetizer as shown in Fig. 1-2.
1. Repeat step 5 for each head stack.
1. Repeat the motions of step 5 for each guide and other metallic parts in the tape path.
1. Move the demagnetizer slowly away from the transport for at least three feet and then disconnect power from the demagnetizer.

Fig. 1-2 Demagnetizing
1-2-(3) LUBRICATION
The only components requiring lubricaiton [sic] are the capstan sleeve bearing and the capstan pinch roller bearings. See Fig. 1-3 and proceed as follows:
CAUTION
BE CERTAIN TO CLEAN CAPSTAN SHAFT THOROUGHLY. THE LUBRICATING OIL CAN RUIN THE CAPSTAN PINCH ROLLER AND MAGNETIC TAPE. CLEAN THE CAPSTAN AND PINCH ROLLER WITH ISOPROYL [sic] ALCOHOL.

Fig. 1-3 Lubrication
1. Unscrew pinch roller cap.
1. Remove pinch roller from the pinch roller shaft.
1. Remove metal dust cap from the capstan shaft by turning counterclockwise.
1. Now the felt collar is visible. Apply 2 or 3 drops of oil onto this felt collar. Please do not over lubricate.
1. Apply a few drops of oil to the pinch roller bearings.
1. Wipe off any excess oil and reinstall the dust cap, pinch roller cap as they were.


SECTION 2 — TAPE TRANSPORT MAINTENANCE
Tape transport maintenance includes procedures for adjusting supply and takeup reel brakes, adjusting supply reel hold-back tension, and adjusting capstan pinch roller pressure.
2-1 TRANSPORT ACCESS
To gain access to recorder transport proceed as follows:
1. Remove power cord and place recorder in an upright position.
1. Use metric allen wrench and remove top panel, two side panels, and rear cover by removing four screws per panel (16 screws total).

Fig. 2-1 Transport Access
2-2 BRAKE ADJUSTMENT
The brake system on each reel stops reel rotation when entering stop mode or when power is removed. The brakes are checked and adjusted with power removed. Since the brake force is different for each direction of rotation (brake differential), and there is a single adjustment, the force is checked and adjusted for the best compromise force in each direction.
In the following steps, an empty 10½ inch diameter NAB reel (4½ inch diameter hub) is used and a cord or twine is wrapped on the reel. A spring scale is attached to a small loop formed in the free end of the cord or twine.
If an [sic] 10½ inch diameter NAB reel (4½ inch diameter hub) is not available, a 7 inch diameter (2¼ inch diameter hub) may be used but all readings must be multiplied by a factor of 2. Proceed as follows: Refer to table 2-1 for the tension specifications on each Model.
1. Place an empty 10½ inch diameter NAB reel on the supply reel turntable. Secure with a holddown knob.
1. Wind a cord or twine a few turns counterclockwise on the hub. Tie a loop in the free end of the cord or twine.
1. Insert the hook of a 0-16 ounce or 0-32 ounce spring scale through the loop and hold the spring scale upright as shown in Fig. 2-2.
1. Pull on the scale slowly to make the reel rotate counterclockwise. While being sure the cord does not rub against either flange, note the scale reading. Reading should be “B” in Table 2-1.
1. Wind the cord or twin [sic] in a clockwise direction on the supply reel.
1. Repeat steps 3 and 4 to make the reel rotate clockwise. Reading should be “A” in Table 2-1.
1. If the readings were low in both directions, remove the brake spring (shown in Fig. 2-3) from the existing anchor hole on the brake lever and install spring in the next hole located farther away from the brake solenoid.
1. If the readings were high in both directions move the spring anchor point to a hole closer to the brake solenoid.
1. If the brake spring was moved, repeat steps 2 through 6 to check results.
1. Repeat the brake adjustment procedure on the takeup reel. Note that the high braking force is present when the takeup reel is rotated clockwise. The tension specifications are the same as for the supply reel.

Fig. 2-2 Measurement
Table 2-1 Tension specifications
	A
	3.6~4.5oz (100~125g)

	B
	7.9~9.7oz (225~275g)



Fig. 2-3 Adjusting Parts Location
2-3 TAPE TENSION ADJUSTMENT
Tape tension is controlled by the amount of torque applied by the reel motors. Only the supply reel motor torque is adjustable. The tape tension is determined indirectly by measuring the supply motor holdback torque in play and fast forward modes. This tension is adjusted by positioning sliders on resistors located below the takeup motor (Fig. 2-4). When adjusting the sliders, loosen the contact screws just enough to slide the contact, then tighten the screw just enough to make good electrical contact.
WARNING
WHEN TRANSPORT POWER IS ON, LINE VOLTAGE IS PRESENT AT THE RESISTORS. TURN POWER OFF BEFORE MAKING AN ADJUSTMENT.
The supply reel tensions were adjusted at the factory with a local power line source. Since motor torque is affected by the source voltage, verify the source voltage is correct before making any adjustment.
In the following steps, an empty 10½ inch diameter NAB reel is used and a cord or twine is wrapped on the reel in the same direction as tape is pulled onto the reel. A spring scale is attached to a small loop formed in the free end of the cord or twine. If an [sic] 10½ diameter NAB reel (4½ inch diameter hub) is not available, a 7 inch diameter (2¼ inch diameter hub) may be used but all readings must be multiplied by a factor of 2. The spring scale is held stationary (Fig. 2-2) and with no slack in the cord. The scale indicates cord tension when in fast forward or play modes. Proceed as follows:
1. Use adhesive tape to hold the takeup-tension-arm safety switch in an upright position so that the safety switch is not activated.
1. Place an empty 10½ inch NAB reel on the supply turntable and secure reel with a holddown knob.
1. Wind the cord or twine a few turns counterclockwise onto the reel hub. Fasten a spring scale to a loop formed on the free end of the cord or twine (Fig. 2-2).
1. Apply power to the recorder.
1. Press F.FWD pushbutton switch. The reading should be “C” in Table 2-2. If necessary adjust slider “C”. (Moving slider towards front of transport increases tension.)
1. Set REEL switch to Large “out” position.
1. Hold the scale upright and press PLAY pushbutton switch. After an initial surge, the reading should be “A” in Table 2-2. If necessary adjust slider “A”. (Moving slider towards front of transport increase [sic] tension.)
1. Set REEL switch to Small “in” position.
1. Press PLAY pushbutton. After an initial surge, the reading should be “B” in Table 2-2. If necessary adjust slider “B”. (Moving slider towards front of transport increases tension.)

Fig. 2-4 Tape Tension Adjustment Resistors
Table 2-2 Tape Tension Specifications
	SLIDER
	MODE
	Specification

	A
	PLAY LARGE
	2.2~2.7 oz (63~77 gram)

	B
	PLAY SMALL
	1.4~1.8 oz (40~50 gram)

	C
	F.FWD.
	1.4~1.8 oz (40~50 gram)


2-4 CAPSTAN PINCH ROLLER PRESSURE ADJUSTMENT
The capstan pinch roller pressure against the capstan is determined by the capstan solenoid spring. This force is adjusted by means of nut shown in Fig. 2-6. This force is adjusted by means of nut shown in Fig. 2-6. [sic] The nut is adjusted to obtain a force of 6.4~7.0 pounds. The resistance of the solenoid coil rises with temperature and causes the solenoid force to decrease. Therefore, do not adjust the pinch roller pressure until the recorder has been operated in play mode for at least 30 minutes prior to performing the following procedure.
1. Use adhesive tape to hold the takeup-tension-arm safety switch in an upright position so that the safety switch is not activated.
1. Tie a cord or twine together for [sic] form a continuous loop. Place one end of the loop around the capstan pinch roller shaft.
1. Press the PLAY pushbutton. The pinch roller will move to contact the capstan and both will rotate.
1. Hook a 0 to 10 pound spring scale to the other end of the cord and pull the cord taut straight to center of capstan as shown in Fig. 2-5. Do not let the cord contact the rotating pinch roller.
1. Pull on the scale and note the scale reading when the pinch roller just loses contact with the capstan (the pinch roller stops rotating). The scale reading should be 6.4~7.0 pounds.
1. If the proper scale reading was not obtained in step 5, loosen the locknut and adjust the pressure nut as required. (Turning the pressure nut towards the spring increases pinch roller pressure.) Tighten locknut.
1. After adjustment is completed, check that the solenoid bottoms within the solenoid coil (pinch roller can easily be pushed away from the capstan). If the solenoid does not bottom, loosen locknut and turn pressure nut away from spring until solenoid bottoms. Recheck pressure adjustment and tighten locknut.
After the proceeding [sic] adjustments are completed, reinstall top panel, two side panels, and rear cover (16 screws total). For transport component replacement procedures, refer to Section 4 of this manual.

Fig. 2-5 Measurement

Fig. 2-6 Adjusting Parts Location
2-5 CAPSTAN SPEED ADJUSTMENT (D Type Only)
Capstan speed can be adjusted by speed control on servo control printed circuit board.
This adjustment follows tape speed measurement in Section 3 and adjust [sic] the speed control as shown in Fig. 2-7 as necessary.

Fig. 2-7 Adjusting Parts Location
Site note: Speed on the first-gen AC transport is set by the mains-locked hysteresis-synchronous motor and the P-12 speed board's 50/60 Hz capacitor values — see Is it a Mini Pro? (https://otarimx5050.com/identify/) for photos of the board.


SECTION 3 — PERFORMANCE TESTS AND ELECTRONIC ALIGNMENT
Performance tests should be performed at regularly scheduled intervals (every 150 hours or 1 month periods) to ensure the recorder is performing within specifications. These tests should also be performed whenever the recorder appears to be malfunctioning and following repairs to the equipment that may affect performance. If the performance test is not successful, proceed to the applicable electronic alignment procedure. It is important that clean and demagnetize the head and tape guiding components before performing the following steps.
Site note: Period measured results for these tests exist: Audio magazine ran them on a 2SH in April 1976 — figures on the specs page (https://otarimx5050.com/specs/).
3-1 TEST EQUIPMENT
The test equipment listed in Table 1-1 is required for completion of the performance and alignment procedures.
3-2 TEST TAPES
The test tapes are precisely recorded under controlled conditions and must be correctly handled and stored to retain their accuracy. The following requirements should be followed:
1. Clean and demagnetize the heads and tape guiding components before installing the test tape.
1. Never store test tapes in areas where there are temperature or humidity extremes.
1. Remove test tapes from equipment only after a normal play run (never after a fast-winding mode). This is further explained below.
During the alignment procedure, the rewind and fast forward modes should not be used. After alignment, wind the tape completely on the takeup reel, interchange reels, thread the tape, and place the equipment in the play mode to wind the tape back on its original reel.
All tones on an Ampex 15 in/s standard alignment tape are recorded at operating level. On slower speed tapes, all tones are recorded 10 dB below operating level except for the last tone. After extensive use, high frequency tones may drop as much as 2 dB. In addition, flutter indications may rise even though actual flutter remains unchanged. Flutter increase is caused by : demagnetization of the recorded signal from repeated plays; tape deformation due to tape tension, changes in temperature and humidity; and increased dropouts resulting from tape wear.
3-3 TEST CONDITIONS
The test conditions specified in the following steps are to be used prior to performing the tests. After these test conditions are set up, continue with the procedures that follow for checking overall signal-to-noise, overall distortion, crosstalk, and flutter.
1. Clean and demagnetize the heads.
1. Use high quality low-noise tape such as Ampex 406, 407, 456 or Scotch 206, 207, 250, or equivalent. Bulk erase the blank tape.
1. Turn power on and allow unit to warm up for 20 minutes.
1. Be sure head cover is installed for all tests.
3-4 PERFORMANCE TESTS
Before making performance test, SRL check, reproduce frequency response check, record level check, monitor level check, overall frequency response check, and SEL/REP level check are necessary. Refer to 3-5 ELECTRONIC ALIGNMENT in this section for checking procedures.
For performance tests, preliminary proceed as follows.
Demagnetize and clean heads and guiding compornents. [sic]
1. Set REEL switch to appropriate position, and set EDIT switch to “out” non edit position.
1. Set LINE OUT switch to H, set each RECORD switch to “in” record position, set each SEL/REP switch to “out” position, and set each MONITOR switch to “out” SOURCE position.
1. Thread a reel of bulk-erased tape onto the transport, set SRL switch to SRL position, and push PITCH CONTROL knob to place fix position.
3-4-(1) OVERALL SIGNAL-TO-NOISE
The overall signal-to-noise test requires an ASA “A” weighted filter to attenuate noise outside of the audible frequency band. The filter is shown in Fig. 3-1 and may be built into a small alumimum box as shown in Fig. 3-1. [sic]
Signal-to-noise depends on SRL calibration, reproduce equalization, bias calibration, and record equalization. Proceed as follows:
1. Connect filter to CH-1 LINE OUT and connect VTVM to the output of filter.
1. Hold TEST OSC pushbutton depressed and adjust CH-1 INPUT LINE control for 0 VU indication on the VU meter.
· (On model MX-5050 2SD2, set reproduce head selector switch at the rear of the head assembly to 2T position.)
· Note VTVM indication, VTVM does not read +4 dBm due to insertion loss of filter.
1. Depress CH-1 MONITOR switch to “in” TAPE position, set CH-1 INPUT LINE and CH-1 INPUT MIC controls to full counterclockwise position. Reset TAPE TIMER to “0000”.
1. Start record mode and record for one minute. Rewind the tape to “0000” indication on the timer.
1. Reproduce the recorded portion and read noise level on VTVM.
1. Signal-to-noise retio [sic] is determined by calculating the difference in readings obtained in step 2 and step 5 plus 9 dB (peak recording level—520 nWb/m—is 9 dB above SRL—185 nWb/m)
1. Repeat step 1 through 6 for the other channels as required, change tape speed to other and check signal-to-noise retio. [sic]
Table 3-1. Signal-to-noise specifications (ASA weighted)
	Models
	2S or 2SD
	4S or 4SD

	15 or 7½
	68dB
	65dB

	3¾
	67dB
	64dB


If signal-to-noise specifications are not obtained, check and adjust following items.
1. SRL caliblation [sic] is incorrect.
1. BIAS/CAL adjustment is incorrect.
1. Reproduce equalization is incorrect.
1. Record equalization is incorrect.
1. Bias buffer adjustment is incorrect.
1. Record and/or reproduce electronics is defective.
1. Head is magnetized
1. Affected with magnetic flux of a motor, a soldering iron or a transformer near the recorder.
Site note: The manual’s own List of Illustrations promises a “Fig. 3-5 Bias Buffer Adjusting Parts” that appears nowhere in the scan — a stale entry, likely from an earlier revision. No figure is missing from this transcription.

Fig. 3-1 ASA “A” Weighted Filter
3-4-(2) OVERALL DISTORTION TEST
For accurately checking distortion it is necessary to use an audio oscillator with less than 0.1% distortion and a wave analyzer with an adjustable bandwidth capability. A wave analyzer with too narrow a bandwidth may make it difficult to measure harmonics due to flutter components within the transport. Instruments that measure total harmonic distortion will be affected by tape and modulation noise in addition to harmonic distortion. To measure overall harmonic distortion proceed as follows:
1. Connect wave analyzer to CH-1 LINE OUTPUT and connect audio oscillator to CH-1 LINE INPUT.
1. Set MONITOR switches to “in” TAPE position, set audio oscillator frequency to 1000 Hz.
1. Set wave analyzer frequency to 1000 Hz, bandwidth to 100 Hz, and mode selector switch to AFC.
1. Start Record mode and adjust CH-1 INPUT LINE control for O VU [sic] on the VU meter.
1. Adjust fine tuning control on the wave analyzer and adjust analyzer input level control for full scale reading of 100%.
1. Change wave analyzer tuning control to 2000 Hz and measure second harmonic content. The second harmonic content should not exceed 0.5%.
1. Change wave analyzer tuning control to 3000 Hz and measure third harmonic content. The third harmonic distortion is dependent upon the type of tape used, accuracy of the BIAS/CAL setting. Typical reading for low noise high output tape is 0.5%: Typical reading for standard output professional grade tape is 0.8%.
1. Repeat step 1 through 7 for channel 2.
If distortion specification is not obtained, check and adjust the following items.
1. SRL caliblation [sic] is incorrect.
1. BIAS/CAL adjustment is incorrect.
1. Head is magnetized.
1. Record and/or reproduce electronics is defective.
3-4-(3) CROSSTALK TEST
It is important that blank bulk-erased tape is used for crosstalk test. To measure crosstalk between channels proceed as follows:
1. Follow the procedure for Overall Distortion Test, steps 1 through 5.
1. Connect wave analyzer from the output of CH-1 to CH-2 LINE OUTPUT.
1. Measure the crosstalk in dB.
· Crosstalk should not exceed Table 3-2. If crosstalk specification is not obtained, record and/or reproduce head alignment (height and tape contact) is incorrect or record or reproduce head is detective. [sic]
Table 3-2. Crosstalk specifications (Between adjacent channels)
	2S or 2SD
	4S or 4SD

	60 dB
	55 dB


3-4-(4) ERASURE TEST
It is important that blank bulk-erased tape is used in erasure test. To measure erasing effect proceed as follows.
1. Follow the procedure for Overall Distortion Test step 1 through 5. A 1000 Hz signal is being recorded at SRL.
1. Set SRL switch to off position and adjust OUTPUT control for -10 VU on VU meter.
1. Adjust INPUT LINE control for O VU [sic] on VU meter and 1000 Hz signal is being recorded at 10 dB above SRL. Continue recording for a few minutes.
1. Remove the audio oscillator.
1. Rewind and reproduce the recorded position.
· VU meter reading should be O VU. [sic]
· Check wave analyzer and readjust as necessary.
1. Press RECORD pushbutton to place recorder in record mode.
· As the tape is being erased, adjust the percent scale on the wave analyzer to read the residual 1000 Hz tone.
1. Repeat the same procedure for other channels.
1. Erasure effect should be more than 65 dB.
If erasure specification is not obtained, check and adjust following items.
1. Erase and/or record head alignment is incorrect. (height, tape contact)
1. Erase head is worn.
1. Erase head surface is dirty.
1. Bias oscillator is detective. [sic]
3-4-(5) TAPE SPEED MEASUREMENT
A flutter test tape is used for measuring tape speed.
Since tape tension affects the tape speed, it is important for accurate measurement that flutter test tape is used to be attached to end of full winded blank tape as Fig. 3-2 and is used with REEL pushbutton to appropriate reel size to be used.
Proceed as follows:
1. Place PITCH CONTROL to fix position and set all RECORD switch to off “out” position.
1. Connect frequency counter to LINE OUT and set MONITOR switch to TAPE position.
1. Set SPEED switch to HI and use test tape to appropriate tape speed.
1. Attach test tape to 10½ inch NAB reel as Fig. 3-2, place test tape onto supply reel table, thread the tape, and set REEL switch to L position.
1. Place recorder in play mode and note reading on frequency counter.
· Reading should be 2994 ~ 3006 Hz (3000Hz ± 0.2%).
1. Repeat procedure for at a point towards the end of the reel, for at 7 inch EIA reel and for at low tape speed.
If speed accuracy is not within ± 0.2%, check and adjust following items.
1. Capstan servo control is incorrect (on 2SD or 4SD).
· Capstan belt is dirty or worn (on 2S or 4S).
1. Capstan motor is defective.
1. Pinch roller tire is worn, or has insufficient pressure.
1. Brakeshoe is contacting brake drum.
1. Tape tensions are incorrect.
1. Power requirement is incorrect.

Fig. 3-2 Using Test Tape
3-4-(6) FLUTTER AND WOW TEST
It is recommended that these checks be made with standard flutter test tapes (See Table 1-2) which are recorded on pricise [sic] equipment to produce less than 0.03% rms flutter. If flutter tapes are not available it is possible to record a 3000 Hz or 3150 Hz signal to be used for a flutter measurement. After recording a section of tape, rewind to the begining [sic] and start the tape in the reproduce mode. Since it is possible for the record mode flutter to either add or subtract from the reproduce mode flutter depending upon the phase relationship, it is necessary to make several passes over the recorded section of tape and average the flutter meter readings.
Flutter meters are sensitive to amplitude modulation that results from poor head-to-tape contact or from signal dropouts. Therefore, clean the heads before making flutter tests.
Test tape method is as follows:
It is important that flutter test tape is used to be attached to end of full winded blank tape as Fig. 3-2, and is used with REEL pushbutton to appropriate reel size to be used.
1. Set all RECORD switch to off “out” position, and on 2SD or 4SD, place PITCH CONTROL to fix psition. [sic]
1. Connect flutter meter to LINE OUT of CH-2 and set the channel MONITOR switch to TAPE position.
1. Set selector switch of flutter meter to NAB weighted position, set SPEED switch to HI and use test tape of appropriate tape speeds.
1. Attach test tape to 10½ inch NAB reel as Fig. 3-2, place test tape onto supply reel table, thread the tape, and set REEL switch to L position.
1. Place recorder in play mode and note reading on flutter meter. Reading should be Table 3-3.
1. Repeat procedure for at a point towards the end of the reel, for at 7 inch EIA reel and for at low tape speed.
Record-playback method is as follows:
1. Connect oscillator signal output of the flutter meter to CH-2 LINE INPUT of the recorder.
1. Connect the LINE OUTPUT of the recorder to the signal input of the flutter meter
1. Set SPEED switch to HI, set SRL switch to SRL position set MONITOR switch to TAPE position, start record mode, and adjust appropriate INPUT LINE control
1. Rewind and reproduce recorded portion, note the flutter and wow on the flutter meter.
1. Check flutter and wow at low tape speed and check at a point towards the end of the reel.
Table 3-3 Flutter and wow specifications
	Tape speed
	Flutter and wow

	15 ips
	0.05 %

	7.5 ips
	0.06 %

	3¾ ips
	0.15 %


Flutter and wow can be caused by any element in the tape path. Excessive flutter and wow may be traced by observing the flutter component on an oscilloscope screen connected to the demodulator output of the flutter meter. If the fluctuation rate observed on the oscilloscope coincides with the rotation elements, such as the supply or takeup reel, capstan or pinch roller, the problem source may be easily traced. Other sources of excessive flutter and wow are:
1. Capstan servo control is defective (on D type).
1. Capstan motor is damaged.
1. Capstan needs lubrication (dry bearing).
1. Tape tensions are incorrect.
1. Brakeshoe is contacting brake drum.
1. Tape reels or tape is defective.
1. Pinch roller tire is worn, has insufficient pressure, or pinch roller solenoid is not bottomed.
1. Pinch roller and capstan are dirty.
3-5 ELECTRONIC ALIGNMENT
If the previous performance tests were not successful, perform the following applicable reproduce and record alignment procedure.
Access to electromic [sic] assembly is as follows: The record/reproduce electronic circuitry is contained on three printed circuit board assemblies (PCB). Access to these PCB may be obtained by removing the base of the cabinet (four screws). Fig. 3-4 shows the location of the various circuits contained on the PCBs.

Fig. 3-3 Access to Electronic Assembly
3-5-(1) REPRODUCE ALIGNMENT
Reproduce adjustment consists of reproduce head azimuth adjustment, reproduce equalization adjustment, maximum reproduce level caliblation [sic] (MRL), and standard reference level (SRL) calibration. Location of each calibration potentiometer control is shown in Fig. 3-4. To adjust the reproduce system, proceed as follows:
1. Lift head cover and demagnetize and clean heads and guides.
1. Set LINE OUT switch to HIGH, set SRL switch to “off” variable position. Set REEL switch to appropriate position, and set EDIT switch to “out” (non edit) position. Set reproduce head selector switch to 2T position for models 2S or 2SD, to 4T position for mosels [sic] 4S or 4SD.
1. Set each RECORD switch to “out” (non record) position, set SEL/REP switches to “out” position, and set MONITOR switches to “out” SOURCE position.
1. Connect VTVM to LINE OUT.

Fig. 3-4 Adjusting Parts Location
3-5-(2) VU METER CALIBLATION [sic]
1. Depress TEST OSC switch and adjust INPUT LINE CONTROL to obtain +4dBm reading on VTVM.
1. Adjust R86 (CH-1) and R186 (CH-2) to obtain OVU [sic] reading on VU meter.
3-5-(3) REPRODUCE HEAD AZIMUTH ADJUSTMENT
It is recommended that reproduce head azimuth adjustment is made at 7½ ips tape speed.
1. Set SPEED switch to appropriate position for 7½ ips and set MONITOR switches to “in” TAPE position.
1. Thread 7½ alignment test tape on the equipment.
1. Place equipment in play mode, first tone on test tape is refference [sic] level of 700 Hz. Adjust OUTPUT level control to obtain O dBm on the VTVM. Next tone is for azimuth adjustment (15 kHz).
1. Adjust the head azimuth screw (appropriate screw “A” in Fig.4-6) to obtain a maximum reading on the VTVM.
CAUTION
DO NOT ADJUST ANY OTHER SCREWS EXCEPT AZIMUTH ADJUSTMENT SCREW (LABELED “A” IN FIG. 4-6).
If a maximum reading cannot be achieved within one full turn of the azimuth screw, or a maximum reading on the VTVM is way below O dBm, a full head alignment may be required. Refer to section 4 of this manual.
3-5-(4) REPRODUCE EQUALIZATION ADJUSTMENT
This adjustment is performed at 7½ ips tape speed for both High speed models and Low speed models.
1. Reproduce the 10 kHz tone and adjust REP EQ potentiometer R60 (CH-1) and R161 [sic] (CH-2) so that VTVM indicate O dBm. If adjustment was required, recheck the 15 kHz tone and note if reading is O dBm ±2 dB.
1. Check response for the other tones on the alignment tape. Frequency response should be O dBm ± 2 dB.
1. Check frequency response for the other tape speed. Frequency response should be O dBm ±2 dB. It is unnecessary to readjust equalization for 15 ips or 3¾ ips, since adjustment has been done at the same time of 7½ ips.
NOTE
Many test tapes are recorded full track. When reproduced by a half-track or multi–track head, the fringing effect produces invalid response at frequencies below 700 Hz. This effect, which results in high indications in the lower frequencies, does not occur when tapes are recorded and reproduced with heads of the same configuration. Do not adjust the low frequency reproduce equalizers for flat response from a full track standard tape.
3-5-(5) MAXIMUM REPRODUCE LEVEL (MRL) CALIBLATION [sic]
This adjustment is performed at 7½ ips tape speed.
1. Set both OUTPUT controls to full clockwise position.
1. Reproduce a 7½ ips alignment test tape. When the first 700Hz tone is reached, adjust maximum reproduce level caliblation [sic] potentiometers R63 (CH-1) and R163 (CH-2) so that each VU meter indicates O VU.
NOTE
The first tone is a reference level which is recorded at 10 dB below operating level (185nWb/m).
3-5-(6) SRL ADJUSTMENT
This adjustment is made with the operating level 700 Hz signal of the standard alignment tape. It is important that this adjustment is accurate since it affects signal to noise ratio, distortion, and tape saturation level. On Ampex standard alignment tapes this level is 185 nWb/m and is the first tone for 15 ips the last tone for 7½ ips and 3¾ ips tapes. It is suggested that SRL be set at the speed at which the equipment will usually run. If used equally, set at 15 ips for high speed models, 7½ ips for low speed models.
Set SRL switch to SRL position. Reproduce the operating level tone and adjust SRL/CAL potentiometers R65 (CH-1) and R165 (CH-2) so that each VU meter indicates O VU or a +4 dBm or -10 dBm reading on the VTVM depending upon the LINE OUTPUT LEVEL selector.
NOTE
If high output extended dynamic range tapes are to be used exclusively such as Scotch 206, 207 or 250 or Ampex 406, 407 or 456 (or equivalent), the SRL/CAL and SEL/REP levels may be set lower than O VU. Consult Otari representative. Nominal setting for these tapes is -3 VU.
3-6 RECORD AND BIAS SYSTEM ADJUSTMENT
Record and bias system adjustment consists of bias calibration, record level calibration, record head azimuth adjustment, record equalization adjustment, and SEL/REP LEVEL adjustment. The record and bias system adjustment should be made after reproduce system adjustments are completed.
1. Connect VTVM to LINE OUT, connect audio oscillator to LINE IN, and thread blank bulk-erased tape onto the transport.
1. Push POWER switch to on, set SPEED switch to HI position, and set MONITOR switch to TAPE position, set LINE OUT LEVEL switch to HIGH position, and SRL switch to SRL position.

Fig. 3-4 Adjusting Parts Location
3-6-(1) BIAS CALIBRATION
Bias adjustment should be made at 15 ips for high speed models and 7½ ips for low speed models. Record bias current affect signal-to-noise ratio, frequency response, distortion, and recording level. Then it is important to adjust bias current for the using tape in order to make perfect recording.
1. Connect 1 kHz tone of audio oscillator to LINE INPUT. (Built in TEST oscillator is also available.) Set MONITOR switch to TAPE position.
1. Start Record mode and adjust INPUT LINE control for O VU on the VU meter.
1. Adjust the BIAS/CAL potentiometers R38(CH-1) and R138(CH-2) so that each VU meter indicates maximum record output.
3-6-(2) RECORD HEAD AZIMUTH ADJUSTMENT
This adjustment should be made at 7½ ips tape speed and at least 10 dB below SRL.
1. Set audio oscillator frequency to 15 kHz.
1. Start record mode and adjust INPUT LINE control for -10 dBm on VTVM (14 dB below SRL).
1. Adjust record head azimuth adjustment screw (labeled “A” in Fig. 4-6) for maximum reading on VTVM.
1. If a peak reading cannot be achieved within one full turn of the azimuth screw, a full head alizument [sic] may be required. Refer to Section 4 of this manual.
3-6-(3) RECORD LEVEL CALIBLATION [sic]
This adjustment should be made at 15 ips for high speed models and 7½ ips for low speed models.
1. Set audio oscillator frequency to 1 kHz, set SRL switch to SRL position, and set MONITOR switches to TAPE position.
1. Start record mode and adjust input LINE controls so that each VU meter indicates O VU.
1. Set MONITOR switches to SOURCE position and adjust REC. CAL. potentiometers R30 (CH-1) and R130 (CH-2) so that each VU meter indicates 0 VU.
3-6-(4) RECORD EQUALIZATION ADJUSTMENT
This adjustment should be performed at SRL position for 15 ips tape speed and at least 10 dB below SRL for 7½ ips or 3 ¾ ips tape speed. Since overall frequency response is affected with bias current, bias calibration may be performed before making this adjustment.
ADJUSTMENT FOR 15 ips
1. Set SRL switch to SRL position, and set MONITOR switches to TAPE position.
1. Place recorder in record mode, set audio oscillator frequency to 1 kHz and adjust INPUT LINE controls for O VU on VU meters.
1. Change frequency to 18 kHz and adjust REC/EQ potentiometers R29 (CH-1) and R129 (CH-2) so that each VU meter indicates O VU.
1. Sweep oscillator frequency from 35 to 22 kHz. Check that the overall frequency response is within ±2 dB. Readjust REC/EQ potentiometers R29 (CH-1) and R129 (CH-2) as necessary.
ADJUSTMENT FOR 7½ ips
1. Set SRL switch to “off” or “variable” position and set OUTPUT controls to full clockwise position.
1. Place recorder in record mode. Set audio oscillator frequency to 1 kHz and adjust INPU [sic] LINE controls for O VU on VU meters (recording is made at 10 dB below SRL).
1. Change frequency to 15 kHz and adjust REC/EQ potentiometers R28 (CH-1) and R128 (CH-2) on high speed models or R29 (CH-1) and R129 (CH-2) on low speed models, so that each VU meter indicates O VU.
1. Sweep oscillator frequency from 30 to 18 kHz and check that the over all frequency response is within ±2 dB. Readjust appropriate REC/EQ potentiometer as necessary.
ADJUSTMENT FOR 3 ¾ ips
1. Set SRL switch to “off” or “variable” position and set OUTPUT controls to full clockwise position.
1. Place recorder in record mode. Set audio oscillator frequency to 1 kHz and adjust INPUT LINE controls for O VU on VU meter (recording is made at 10 dB below SRL).
1. Change frequency to 10 kHz and adjust REC/EQ potentiometers R28 (CH-1) and R128 (CH-2) so that each VU meter indicates O VU.
1. Sweep oscillator frequency from 30 to 12 kHz and check that the over all frequency responce [sic] is within ±2 dB. Readjust appropriate REC/EQ potentiometer as necessary.
3-6-(5) SEL/REP LEVEL ADJUSTMENT
1. Record 1 kHz signal at SRL for about one minute for both channels.
1. Rewind and reproduce the recorded position in the step, and check both VU meters should indicate O VU.
1. Depress SEL/REP switch and adjust SEL. REP LEVEL potentiometers R367 (CH-1) and R387 (CH-2) so that each VU meter indicates O VU.
NOTE
If this adjustment is made by using standard alignment test tapes which are full track recorded, there will be a little error on acount [sic] of fringing effect.


SECTION 4 — MAJOR COMPONENT REPLACEMENT PROCEDURES
4-1 TAPE TRANSPORT
In order to gain access to the tape transport components, place the recorder in an upright position and remove rear cover, two side panels, and top panel (16 screws total).
Refer to Section 6 for parts lists and exploded views of the transport assembly to aid in the identification of the various components.
4-1-(1) REEL TABLE REPLACEMENT AND HEIGHT ADJUSTMENT
The reel table may be removed by removing three cross head screws accessible from the front of the transport. To adjust the reel table height, loosen two hexagonal socket head screws shown in Fig. 4-1, adjust height and retighten screws.

Fig. 4-1 Reel Table and Motor
4-1-(2) SUPPLY OR TAKEUP REEL MOTOR REPLACEMENT
To replace the supply or takeup motor proceed as follows:
1. Loosen two hexagonal socket head screws on the reel shaft holder (Fig. 4-1) and remove reel table and holder.
1. Tag and unsolder motor leads from the attached printed circuit board.
1. Remove four motor mounting M4 nuts.
1. Remove four motor mounting crosshead screws.
1. Install new motor in the reverse order of removal and adjust reel table height.
4-1-(3) POWER TRANSFORMER REPLACEMENT
To replace the power transformer (refer to EXPLODED VIEW 2), proceed as follows:
1. Tag and unsolder all transformer leads from the terminal.
1. Remove four M4 nuts that secures [sic] the transformer to the transport. (Ref. No. 2-18)
1. Install new transformer in the reverse order of removal and resolder leads to the terminal of the transformer.
4-1-(4) CAPSTAN MOTOR REPLACEMENT
On models 2S or 4S (Hysteresis synchronous motor machines).
To place [sic] the capstan motor (Fig. 4-1 and refer to Exploded View 4), proceed as follows:
1. Tag and unsolder all motor leads from the printed circuit board.
1. Remove entire motor assembly and mounting bracket by removing four cross head screws accessible from the rear of the transport.
1. Remove motor pully [sic] from motor shaft by loosening an allen head screw.
1. Remove motor from mounting bracket and replace with new motor.
1. Reinstll [sic] motor assembly and mounting bracket in the reverse order of removal. Adjust bracket position to tighten drive belt before cross head mounting screws are tightened.

Fig. 4-2 Capstar Motor Location (2S or 4S)
On models 2SD or 4SD (DC servo controlled motor machines)
The capstan motor should be replaced with servo control printed circuit board assembly, to replace the capstan motor proceed as follows: (Refer to EXPLODED VIEW 4-2)
1. Remove connector on servo control printed circuit board assembly located above capstan.
1. Remove servo control printed circuit board assembly with mounting plate by turning four M3 crosshead screws “B” on mounting plate.
1. Remove capstan dust cap from face of transport. (Ref. No. 4-102)
1. Remove capstan mounting plate with capstan motor by removing four M4 crosshead screws “A” on the mounting plate.
1. Remove the capstan motor by removing three M4 crosshead screws “C” on the mounting plate and install new capstan assembly in the reverse order.

Fig. 4-3 Capstar Motor Location (2SD or 4SD)
Site note: Exploded view 4-1 is the AC belt-drive capstan with its run cap; 4-2 is the DC-servo capstan of the 2SD/4SD variants — the detail that settled which machines the DC sections of this manual describe. Replacing the run caps is written up in Re-capping the motor run caps (https://otarimx5050.com/log/recapping-motor-run-caps/).
4-1-(5) BRAKE BAND OR BRAKE SOLENOID REPLACEMENT
When a new brake band or new brake solenoid is installed (Fig. 2-2), it is necessary to position the brake guide and/or brake solenoid to ensure that there is uniform brake band clearance around the brake drum when the solenoid is energized. Also the brake solenoid plunger must bottom in the solenoid housing when the solenoid is energized. When the solenoid is deenergized, the brake band should uniformally [sic] contact the drum surface. After installation, perform the Brake Adjustment procedure given in Section 2 of this manual. After completion of the adjustments place the recorder in play mode for 30 minutes. Then press STOPand [sic] PLAY pushbuttons to ensure that the solenoid bottoms when it is hot.
Site note: The transport push-buttons and their microswitches are documented with part numbers and photos in Inside the transport buttons (https://otarimx5050.com/log/transport-buttons/).

Fig. 4-4 Brake Assembly Location
To replace the brake band or brake solenoid, proceed as follows:
1. Remove brake spring and retaining ring “A”.
1. Remove retaining ring “B” of solenoid pin. [sic] and remove solenoid pin.
1. Remove solenoid housing with plunger by removing two hexagonal socket head screws.
1. Install new solenioid [sic] housing with plunger and set solenoid housing so that plunger stroke is 0.2 ± 0.02 inch (5 ± 0.5 mm).
1. Remove spring pin of brake lever and remove brake band by removing two cross head screws.
1. Install new brake band in the reverse order.
4-1-(6) PINCH ROLLER REPLACEMENT
To replace the pinch roller assembly proceed as follows:

Fig. 4-5 Pinch Roller Removal
1. Remove pinch roller cap by turning counterclock wise [sic].
1. Install new pinch roller.
1. Reinstall nylon washer and pinch roller cap in the reverse order.
4-2 HEAD ASSEMBLY REPLACEMENT
This section provide [sic] a description of the head assembly, procedures for changing head stacks and adjustment procedures for adjusting head azimuth (tilt), head height, head zenith (perpendicularity) and tape wrap (racking). These adjustments are required whenever a head stack is replaced.
NOTE
AFTER HEAD ALIGNMENT, ALIGNMENT SCREWS (AZIMUTH, ZENITH, HEIGHT) SHOULD BE LOCKED UP WITH ENAMEL PAINT.
DESCRIPTION
The head assembly is mounted on three tape-guide posts and secured in place by three screws labled [sic] “M” in Fig. 4-6.
The insulating shield for the head assembly printed circuit board is secured by screws labled [sic] “S”. Each head stack is secured to a bracket by screws labled [sic] “W” with a spacer between the bracket and head stack. Each bracket is suspended from the head base by three spring-loaded screws labled [sic] “H”, “A”, and “Z”. Screws labeled “W” are used to adjust tape wrap. Screws labeled “H”, “A”, and “Z” are used to adjust height, azimuth, and zenith.
A head stack may be removed and re-lapped (face resurfaced) if the amount of wear is small and only an indication of poor head-to-tape contact is evident. Poor contact is a result of improper adjustment and is evidenced by loss of high frequency response of the record or reproduce head stack, difficulty in achieving bias peak (record stack), or insufficient erase stack erasure.
HEAD STACK REPLACEMENT
To change a head stack, proceed as follows:
1. Lift head cover, remove AC power cord.
1. Remove three screws labeled “M” and pull out the head assembly from head connector.
1. Tag and unsolder (use low wattage pencil type iron to prevent damage) leads at rear terminal of the head stack.
1. Remove head stack by removing two screws labeled “W”.
1. Install new head stack and resolder leads.
1. As a preliminary adjustment, measure the distance between the head base and the bracket at a point near spring-loaded screws “A”, “Z”, and “H”. If necessary adjust screws for equal spacing.
1. Lay a piece of ¼-inch tape over the spacers and head stacks as shown in Fig. 4-7. Note if the leading and trailing wrap angle around the head stack is equal. If not equal, correct by loosening screw “W”, adjusting head stack, and retightening screws. Remove the three screws and spacers installed in step 7.
1. Remount the head assembly. Perform the appropriate head alignment procedure given below.
Following adjustment are [sic] necessary whenever head is replaced.
1. In case of reproduce head replacement. A. Reproduce Equalization Adjustment (See 3-5-([illegible]) ) B. SRL Calibration (See 3-5-(6) )
1. In case of record head replacement. A. Bias Calibration (See 3-6-(1) ) B. Record Level Calibration (See 3-6-(3) ) C. Record Equalization Adjustment (See 3-6-(4) ) D. SEL/REP Level Adjustment (See 3-6-(5) )
1. In case of erase head replacement A. Bias Calibration (See 3-6-(1) )
Site note: The cross-reference digit is unreadable in the scan; Section 3’s own numbering shows Reproduce Equalization Adjustment as 3-5-(3).
RECORD OR REPRODUCE HEAD ADJUSTEMNT [sic]
Follow the procedure for Reproduce Amplifier Alignment given in Section 3 of this manual. For the final adjustment of a record stack, the height and azimuth adjustment may be accomplished in the same manner as for a reproduce head stack by playing back an alignment tape with the recorder in the selective reproduction mode (SEL/REP switches “in”). Use the 10 kHz tone for azimuth adjustment.
ERASE HEAD ALIGNMENT
Erase head azimuth is not critical, however wrap angle and head height relative to the record head is important to achieve maximum efficiency. Poor erasure is often caused by misalignment of the erase head. Before making any attempt to adjust the erase head stack, an entire electronic alignment procedure (reproduce, record, and bias amplifier alignment) should be performed so that the record and reproduce head heights are correct, SRL/CAL setting is correct, and bias and record levels are properly calibrated. If [sic] should be also noted that in some cases, high coercivity tape can be the cause of poor erasure.
An approximate erase head adjustment can be accomplished using headset or a speaker/amplifier. However, for precise alignment, a wave analyzer should be used. Proceed as follows:
1. Follow the procedure for Erasure Test steps 1 through 6 given in Section 3 of this manual.
1. Observe reading on wave analyzer and turn screw “H” (Fig.4-5) ¼ turn clockwise. If the reading decreased, turn screw “A” and “Z” ¼ turn clockwise. If the reading increased when “H” was turned ¼ turn clockwise, turn “H” counterclockwise past the original setting to ¼ turn counterclockwise. If the reading decreased, turn screw “A” and “Z” counterclockwise by the same amount.
1. Repeat step 2 in small increments to achieve a minimum reading on the wave analyzer. Typical amount of erasure should be 65 dB or better. Note: After “H” is turned, be sure to turn “A” and “Z” the same amount.
1. If the adjustment of erase head height alone cannot achieve satisfactory erasure, set screw “H”, “A”, and “Z” for minimum reading on the wave analyzer. Note that there are two vertical gaps on the face of the erase head. The trailing gap has the most effect on erasure and must be in good contact with the tape. Loosen screws “W” slightly and rotate the erase head stack for a minimum reading on the wave analyzer. Tighten screws “W”.

Fig. 4-6 Top View of Head Assembly

Fig. 4-7 Front View of Head Assembly

Fig. 4-8 Bottom View of Head Assembly

Fig. 4-9 Head Alignment
4-3 INSTALLATION OF OPTIONAL TRANSFORMER
4-3-(1) INSTRUCTION OF INPUT TRANSFORMER
Follow the instruction to install the input transformer.

Fig. 4-10 Input Circuity
Input transformer has terminals as shown above surrounded by broken line.
1. Take out case rear board as shown in Fig. 2-1, and out Rear Panel [sic]. Then mount the transformer with two screws. (See Fig. 4-12)
1. Remove wires from XLR connector. Solder Hot Line (Orange) to transformer output side number 5, Solder Cold Line & Shied [sic] to terminal number 8.
1. Solder Hot Line (Orange) premounted on the transformer to XLR connector number 3, Cold Line (White) to XLR connector number 2, and Shield to XLR connector l [sic]. (See Fig. 4-13)
1. Take out the bottom board and re-wire the PCB as shown below.

Fig. 4-11 P.C. Board Wiring
A Take out jumpers 1 and 2 . B UM-solder [sic] 3 and solder to 5. C UM-solder [sic] 4 and solder to 6.

Fig. 4-12 Input Transformer Installation

Fig. 4-13 Input Transformer Wiring
1. After all of above modification, please test record.
4-3-(2) INSTALLATION OF OUTPUT TRANSFORMER
Fig. 4-15 [sic] shows circuity of unbalanced output and balanced output. To install input transformer [sic], proceed as follows:

Fig. 4-14 Output Circuity
Transformer has terminals as shown above surrounded by broken line.
1. Take out case rear board in the Fig. 11-1 [sic], and then take off rear panel. Mount the transtormer [sic] with two screws.
1. Remove wires from XLR connectors. Solder Hot Line (Orange) to transformer terminal 1, and Solder Cold Line (White) and Shield to terminal 2.
1. Solder Orange Wire coming out of terminal 5 to XLR connector number 3, Solder White Wires coming out of terminal 8 to XLR connector number 2, Solder Shield Wire to XLR connector number 1.
1. After above wiring, put test tape and adjust reproduce level.

Fig. 4-15 Output Transformer Installation

Fig. 4-16 Output Transformer Wiring


SECTION 5 — TROUBLESHOOTING
5-1 PRELIMINARY PROCEDURES
If a problem should occur with the recorder, check that the following items are correct before proceeding with troubleshooting procedures. As an aid in troubleshooting, refer to the schematic diagram and parts lists included in this manual.
1. Head stacks are cleaned and demagnetized.
1. Head azimuth and height are correct.
1. Record bias has been adjusted properly.
1. Recommended tape has been used.
1. Input and/or output connectors are correctly wired.
1. Ac line voltage is within ± 10% of indicated power requirement.
1. All operational switches have been correctly set.
1. Adjustment procedures have been correctly made using accurate test equipment.
5-2 TROUBLESHOOTING HINTS
Some of the more common problems and possible causes are listed in Table 5-1.
Site note: Before chasing anything in this table: if the transport is completely dead, check the rear REMOTE socket — the machine needs a remote or a dummy plug there. Mine was “broken” for exactly this reason: No dummy plug — no problem! (https://otarimx5050.com/log/building-a-dummy-plug/).
Table 5-1 Troubleshooting Hints
	SYMPTOM
	POSSIBLE CAUSE

	Power switch is on but meters do not illuminate and transport does not function.
	Fuse is blown, ac power cord is defective, or power switch is defective.

	Transport function and meters illuminate but no recording and reproducing
	Power source for amplifier (+29Vdc)’ [sic] is defective.

	Transport does not function.
	Power source for control (+24Vdc) is defective.

	Capstan shaft does not rotate
	Tension arm safety switch is defective. On models 2S or 4S, capstan motor is defective or capstan belt come off[sic]. On Models 2SD or 4SD, power source for capstan motor (+24Vdc or +5Vdc) is defective, or fuse of the power supply is blown.

	No PLAY mode function
	Control circuit (PA-284) is defective (Tr8,9,SCR2,3))[sic], or pinch roller solenoid is defective.

	No FAST FORWARD mode function
	Control circuit (PA-284) is defective (Tr 3,4, SCR 1).

	No REWIND mode function
	Control circuit (PA-284) is defective (Tr2).

	Record lamp of transport does not illuminate and no RECORD mode function
	Control circuit (PA-284) is defective (Tr10, SCR4)

	Brake solenoide[sic] does not move.
	Control circuit (PA-284) is defective (Tr5), or brake solenoi–lenoide[sic] is defective, or brake adjustment is incorrect (strok)[sic].

	Tape speed is incorrect
	Pinch roller adjustment is incorrect (not bottomed), or dirty pinch roller, dirty capstan shaft. On models 2S or 4S, loose or dirty capstan belt slips, or capstan motor is defective. On models 2SD or 4SD; capstan servo control circuit is defective, or adjusted incorrectly. Pitch control nob[sic] is at wrong position.

	Output level is wrong
	Reproduce head switch is at wrong position, or output level switch is wrong position.




SECTION 6 — PARTS LISTS AND SCHEMATICS
Site note: The New No. column on the parts lists below is not in the scan this transcription was made from — its column is blank there. The numbers come from my own paper copy, scanned at 1200 dpi and available on the manuals page (https://otarimx5050.com/library/manuals/): a later factory revision that fills the column with Otari’s old-to-new part renumbering. Each cell was transcribed and verified against that scan.
PARTS LIST 1
	Ref. No.
	Description
	Parts No.
	New No.

	1-1
	Left Side Board
	CS-245-004
	K100603

	1-1
	Right Side Board
	CS-245-004
	K100603

	1-3
	Case Top Board
	CS-245-002
	K100601

	1-4
	Cooling Cover
	CS-232-007
	K100602

	1-5
	Case Bottom Board
	CS-245-007
	K100604

	1-6
	Case Rear Board
	CS-245-009
	K1006-D

	1-7
	Rubber Pad
	NB-91-032
	CY4006

	1-8
	Catcher
	CS-245-005
	CY1004

	1-9
	Display Washer
	TY-800-014
	KZ6C016

	1-10
	Sheet
	TY-800-017
	K6C011

	1-11
	Display Washer
	TY-800-021
	KZ6C010



EXPLODED VIEW 1
PARTS LIST 2
	Ref. No.
	Description
	Parts No.
	New No.

	2-1
	Display washer
	TY-800-021
	KZ6C010

	2-2
	Sheet
	TY-800-017
	KZ6C011

	2-3
	Control Display Panel
	TD-5050-004
	T505003

	2-4
	Plain Washer
	TY-800-024
	KZ6C009

	2-5
	Display Panel
	TD-5050D-001(2SD,4SD)TD-5050-001(2S,4S)
	T506006T505002

	2-6
	Amplifier Display Panel
	AF-230-003
	A101601

	2-7
	Amplifier Mounting Base
	AF-230-004
	A101602

	2-8
	Mounting Base
	TD-5010-001
	T505001

	2-9
	Frame
	TD-5010-006
	T505004

	2-10
	Frame Stud
	TD-5010-008
	KZ7B202

	2-11
	Stud
	ST-107
	KZ7A217

	2-12
	Control PCB Assembly
	PA-284
	PB-41D

	2-13
	Power Transfomer [sic]
	ET-11-194
	TF11012

	2-14
	W-W Resistor
	RS-39-40HAAC-600ohm
	RV5J6011

	2-15
	W-W Resistor
	RS-39-30HAAC-200ohm
	R55J2011

	2-16
	Rear Panel
	AF-230-007
	A101609

	2-17
	Rear Name Plate
	AF-230-009
	A101610



EXPLODED VIEW 2
PARTS LIST 3
Site note: The revision’s Parts No. column prints two slash-joined values for 3-2 and 3-3 — “TW-424-001/KW4J002” and “TW-424-002/KWOB017S” — and draws a bracket on the right joining those two lines into one assembly. Read literally: 3-2 (Reel Table) is now sold only as part of that assembly (its New No. cell prints “Assy.#”), and 3-3 (Reel Shaft Holder) carries the assembly’s own new number, KW4J001. Transcribed as printed, not reinterpreted.
	Ref. No.
	Description
	Parts No.
	New No.

	3-1
	Reel Clamper
	TW-661
	TW-670

	3-2
	Reel Table
	TW-424-001
	Assy.#

	3-3
	Reel Shaft Holder
	TW-424-002
	KW4J001

	3-4
	Reel Protector
	TW-424-009
	KW0H007

	3-5
	Counter Grille
	TD-5500-005
	SR8B003

	3-6
	Display Panel
	TD-5050D-001(2sD,4SD)TD-5050-001(2S,4S)
	T505006T505003

	3-7
	Mounting Base
	TD-5010-001
	T505001

	3-8
	Spacer
	TZ-131-001
	SR8B002

	3-9
	Tape Counter
	CT-09-T4A SPEC
	SR-8B

	3-10
	Counter Supporter
	TZ-126-001
	SR8B001

	3-11
	Switch Bracket
	PA-282-003
	T505005

	3-12
	Rotary Switch(With Pulley)
	SW-99-HZR0036-01-010
	WH91005

	3-13
	Endless Belt
	TB-5147-20
	BE1B147

	3-14
	Reel Motor Supporter
	TW-421-018
	KW0G016

	3-15
	Reel Motor
	EW-506-019
	MR1C005

	3-16
	Relaying PCB
	PM-678
	PB9A027

	3-17
	Electrolytic Capacitor
	CD-99-MPL-5.5µ
	CZ10014W

	3-18
	Capacitor Holder
	TW-421-017L
	KW4B003

	3-19
	Capacitor Holder
	TW-421-017R
	KW4B004

	3-20
	Brake Base
	TW-421-009
	KW0G013

	3-21
	Brake Base
	TW-421-007
	KW0G012

	3-22
	Switch Supporter
	TW-421-006
	KW4B002

	3-23
	Spacer
	TW-421-019
	KW4B005

	3-24
	Micro Switch
	SW-59-SS5GL
	WH51002

	3-25
	Brake Guide
	TW-421-004
	KW4B001

	3-26
	Spring
	SG-100-052
	GS1024

	3-27
	Brake Arm
	TW-424-008
	KW0D014

	3-28
	Retaining Ring
	EZ-09-E-15
	F74TE15

	3-29
	Brake Band Assembly(With Sheet)
	……
	KW-4E-A

	3-30
	Pin
	EZ-09-316
	F63316

	3-31
	Brake Drum
	TH-424-007
	KW0A012

	3-32
	Retaning Ring [sic]
	EZ-09-E-9
	F74TE09

	3-33
	Solenoid Pin
	TY-400-015
	MR5A003

	3-34
	Solenoid
	SO-334 DC24V
	GP1F01

	3-35
	Cord Clamper
	………….
	KZ3A047



EXPLODED VIEW 3
PARTS LIST 4-1
	Ref. No.
	Description
	Parts No.
	New No.

	4-1
	Dust Cap
	TC-423-007
	KC0B008

	4-2
	Felt Collar
	TC-419-004
	PZ1B007

	4-3
	Display Panel
	TD-5050-001
	T505002

	4-4
	Mounting Base
	TD-5010-001
	T505001

	4-5
	Metal Holder Assembly
	TC-423-004
	KC4B001

	4-6
	Slide Washer
	TY-800-026C
	KZ6C014

	4-7
	Capstan-Flywheel
	TC-423-001
	KC0A020

	4-8
	Endless Belt
	TB-9140-10-High speedTB-9137-10-Low speed
	BE2M140BE2M137

	4-9
	Stud
	ST-076
	KZ9I755A

	4-10
	Flywheel Holder
	TC-419-007
	KC4B004

	4-11
	Motor Pulley A
	TC-423-008A 50HZ High speedTC-426-001A 50HZ Low speed
	KC0D010KC0D016

	4-12
	Motor Pulley B
	TC-423-008B 60HZ High speedTC-426-001B 60HZ Low speed
	KC0D011KC0D017

	4-13
	Motor Stud
	ST-054
	KZ9I570A

	4-14
	Shielding Plate
	TC-419-012
	KC4B006

	4-15
	Motor Suppoter [sic]
	TC-423-009
	KC4B005

	4-16
	Motor
	EM-408-011
	MR2F010

	4-17
	Electrolytic Capacitor
	CD-99-MPL-2.0+0.5
	CZ10011W

	4-18
	Relaying PCB
	PM-669
	PB9A026



EXPLODED VIEW 4-1 (For Models 2S and 4S)
PARTS LIST 4-2
	Ref. No.
	Description
	Parts No.
	New No.

	4-101
	Knob
	NB-31-037
	KN1013

	4-102
	Dust Cap
	TC-423-007
	KC0B008

	4-103
	Display Panel
	TD-5050D-001
	T505006

	4-104
	Mounting Base
	TD-5010-001
	T505001

	4-105
	Variable Resistor Supporter
	TC-427-003
	KZ2A030

	4-106
	Variable Resistor
	VR-29-EVH-Y03R25B52
	RV252009

	4-107
	+5Volt Dc Power Supply PCB Assembly
	PA-426
	PB-61D

	4-108
	PCB Supporter
	TY-200-082
	KZ3A027

	4-109
	Stud
	ST-086
	KZ7B220

	4-110
	Motor Supporter
	TC-212-001
	KC2B001

	4-111
	Capstan Drive Motor
	EM-710-007A
	MR5A001

	4-112
	Radiator
	TC-212-002
	KZ1A012

	4-113
	PCB Supporter
	TC-427-004
	KZ3A028

	4-114
	Power Supply PCB Assembly
	PA-377
	PB-61E

	4-115
	Fuse Holder
	FS-89-F-3294
	FH1-022

	4-116
	Fuse
	FS-19-2A
	FH7A020


Site note: The revision adds this note beneath the table, verbatim, including what reads as a factory typo — “OF” where “IF” is meant: “THERE ARE VERY FEW OF THIS VERSION IN THE U.S. PLEASE CONFIRM THESE PART NUMBERS WITH THE CUSTOMER OF [sic] THEY ARE ORDERED.” (This crop is pulled from the later-revision 1200 dpi scan, p. 69 — not the 34 MB mirror pagination used for every other correction crop in this file.)

EXPLODED VIEW 4-2 (For Models 2SD and 4SD)
PARTS LIST 5
	Ref. No.
	Description
	Parts No.
	New No.

	5-1
	Pinch Roller Cap
	TP-416-001
	KP0C005

	5-2
	Polyslider Washer
	EZ-09-5TW-FT-6 0.25
	6x0.25 polyslide washer

	5-3
	Pinch Roller
	TP-416-001
	KP0A007

	5-4
	Retaining Ring
	EZ-09-E-20
	F74TE20

	5-5
	Pinch Roller Shaft
	TP-416-002
	KP0B010

	5-6
	Cue Lever
	TR-416-001
	KP0C005

	5-7
	CUE Lever Escutcheon
	TR-416-002
	KR4B006

	5-8
	Display Panel
	TD-5050D-001(2SD,4SD)TD-5050-001(2S,4S)
	T505006T505002

	5-9
	Mounting Base
	TD-5010-001
	T505001

	5-10
	Arm Shaft
	TR-413-002
	KR4B001

	5-11
	Shifter Arm A
	TR-413-003
	KR0B005

	5-12
	Polyslider Washer
	EZ-09-STW-FT-4 0.25
	4x0.25 polyslide washer

	5-13
	Shifter Arm B
	TR-413-007
	KR0B006

	5-14
	Retaining Ring
	EZ-09-E-15
	F74TE15

	5-15
	Spring
	SG-100-050
	GS1028-A

	5-16
	Arm Shaft
	TR-414-003
	KR4B007

	5-17
	Cue Arm
	TR-416-003
	KR4B008

	5-18
	Arm Shaft
	TE-416-002
	KR4B006

	5-19
	Pinch Roller Arm
	TP-420-002
	KR4E001

	5-20
	Arm Guide
	TR-414-007
	KR4B011

	5-21
	Roller Catch
	EZ-09-C-51-2
	CY3001

	5-22
	Retaining Ring
	EZ-09-E-9
	F74TE09

	5-23
	Solenoid Pin
	TY-400-015
	KZ5A003

	5-24
	Solenoid
	SO-317
	GP1B02

	5-25
	Adjusting Rod
	TP-416-009
	KZ6A022

	5-26
	Stopper
	TY-200-013
	KZ2A015

	5-27
	Plain Washer
	EZ-09-M4
	M4 Washer

	5-28
	Retaining Ring
	EZ-09-E-15
	F74TE15

	5-29
	Spherical Washer
	TP-401-007
	KP0G004

	5-30
	Pressure Spring
	SG-500-031
	GS2003

	5-31
	Double Nuts
	EZ-09-M4
	M4 Double Nut

	5-32
	Spring Holder
	TY-900-019
	KZ3A023

	5-33
	Spring
	SG-100-048
	GS1011

	5-34
	Switch Braket [sic]
	TD-500-095
	KZ3A026

	5-35
	Leaf Spring Switch
	SW-09-PU-3024
	WH91004


Site note: Ref. 5-7’s row carries an asterisk in the revision, tied to a footnote below the table, transcribed verbatim: “* Old Part Number is incorrect, new number is correct.”

EXPLODED VIEW 5
PARTS LIST 6
	Ref. No.
	Description
	Parts No.
	New No.

	6-1
	Name Plate
	TH-446-005
	PT1004

	6-2
	Splicing Block
	TH-446-004
	KH4C003

	6-3
	Head Housing Assy
	TH-446-00B
	KH-4C-A

	6-4
	Switch Name Plate
	TH-446-006
	PT4124

	6-5
	Protector Sheet
	TH-438-009
	KH4C002

	6-6
	Head Cord PCB Assembly
	PA-274
	PB-71B

	6-7
	Blind
	TY-900-009
	PZ1B010

	6-8
	Head Base
	TH-446-001
	KH0C011

	6-9
	Head Adjusting Spring
	SG-500-063
	GS2007

	6-10
	Head Supporter B
	TH-422-002
	KH0D005

	6-11
	Head Supporter A
	TH-422-001
	KH0D004

	6-12
	Record Head(2T 2C)Record Head(4T 2C)
	SH-6202-11-001 (2s typs)SH-6204-11-001 (4s typs)
	GH4R005GH4R003

	6-13
	Reproduce Head(2T 2C)Reproduce Head(4T 2C)
	SH-7202-11-001 (2s typs)SH-7204-11-002 (4s typs)
	GH4P006GH4P069

	6-14
	Erase Head(2T 2C)Erase Head(4T 2C)
	SH-5202-11-001 (2s typs)SH-5204-11-001 (4s typs)
	GH4E004GH4E009

	6-15
	Reproduce Head(4T 2C) [sic]Reproduce Head(2S 2C)
	SH-7204-11-001 (2s typs)SH-7204-11-001 (4s typs)
	GH4P069GH4P006

	6-16
	Tape Guide
	TH-438-004
	KG4C002

	6-17
	Housing Base
	TH-438-005
	KH4C001

	6-18
	Push Button A
	CR-824-001A
	KN2020

	6-19
	Push Button C
	CR-824-001C
	KN2022

	6-20
	Push Button B
	CR-824-001B
	KN2021

	6-21
	Push Button E
	CR-824-001E
	KN2024

	6-22
	Push Button C
	CR-823-001C
	KN2018

	6-23
	Push Button B
	CR-823-001B
	KN2017

	6-24
	Push Button D
	CR-823-001D
	KN2019

	6-25
	Push Button A
	CR-823-001A
	KN2016

	6-26
	Control Display Panel
	TD-5050-004
	T505003

	6-27
	Lamp Cover
	TY-900-024 (A:Red,B:Green)
	LU9002

	6-28
	Display Panel
	TD-5050D-001(2SD,4SD)TD-5050-001(2S,4S)
	T505006T505002

	6-29
	Mounting Base
	TD-5010-001
	T505001

	6-30
	Plain Washer
	EZ-09-M4
	M4 Washer

	6-31
	Lamp Supporter
	TY-900-025
	KZ2A029

	6-32
	Lamp Assembly
	PL-19-005
	LU2003

	6-33
	Guide
	CR-823-010
	CB20602

	6-34
	Switch Base
	CR-823-008
	CB20601

	6-35
	Micro Switch
	SW-59-V-1A
	WH11007

	6-36
	2P Terminal
	LP-09-1L2P
	CN902002

	6-37
	Guide
	CR-824-006
	CB20701

	6-38
	Switch Base
	CR-824-005
	PB41E01

	6-39
	POwer Switch PCB Assembly [sic]
	PA-288
	PB-41E

	6-40
	Micro Switch Supporter
	CR-824-007R
	PB41E02

	6-41
	Micro Switch
	SW-59-SS5GL
	WH51002

	6-42
	Switch Supporter
	CR-824-008
	PB41E04


Site note: Ref. 6-27’s row is asterisked in the revision; the New No. cell above (LU9002) is only for the “A:Red” variant already printed in the Parts No. cell. A footnote below the table, keyed by the same asterisk, gives the “B:Green” variant’s new number, transcribed verbatim: “* B:Green … LU9003”
Site note: The transport-button microswitches turn up as Omron V-series parts — V-10-1A8 and V-15-1A5 — and the V-15-1A5 is still in production; marking photos in Inside the transport buttons (https://otarimx5050.com/log/transport-buttons/).

EXPLODED VIEW 6
PARTS LIST 7
	Ref. No.
	Description
	Parts No.
	New No.

	7-1
	Display Screw
	TA-420-005
	KA0C002

	7-2
	Tape Guide
	TA-420-004
	KG4D006

	7-3
	Tension Arm
	TA-420003
	KA0A005

	7-4
	Arm Shaft
	TA-429-001
	KA0A004

	7-5
	Polyslider Washer
	EZ-09-STW-FT-5 0.5t
	5x.5t polyslide washer

	7-6
	Arm Holder
	TA-420-002
	KA0B003

	7-7
	Roller Cap
	TG-424-01
	GR0A005

	7-8
	Polyslider Washer
	EZ-09-STW-FT-8 0.25t
	8x.25t polyslide washer

	7-9
	Roller Shaft
	TG-424-02
	GR4H001

	7-10
	Sleeve
	TG-424-03
	Assy. #

	7-11
	Roller
	TG-424-04
	GR4H002

	7-12
	Roller Base
	TG-424-05
	GR4B004

	7-13
	Display Panel
	TD-5050D-001(2SD, 4SD)TD-5050-001(2S,4S)
	T505006T505002

	7-14
	Mounting Base
	TD-5010-001
	T505001

	7-15
	Micro Switch
	SW-59-1V-3H-2A
	WH51004

	7-16
	Magnetic Supporter
	TY-900-023
	KZ3A025

	7-17
	Spring Holder
	TY-900-020
	KZ3A024

	7-18
	Nut
	TA-420-007
	KZ6D004

	7-19
	Polyslider Washer
	EZ-09-STW-FT-5 0.5t
	5x.5t polyslide washer

	7-20
	Arm Boss B
	TA-427-001
	KA0E005

	7-21
	Spring
	SG-100-047B
	GS1027

	7-22
	Switch Arm
	TA-423-002
	KA4B001

	7-23
	Arm Boss A
	TA-429-002
	KA0E004

	7-24
	Spring
	SG-100-046
	GS1025

	7-25
	Stopper Arm
	TA-420-010
	KA0H004


Site note: As with Ref. 3-2/3-3, Ref. 7-10 and 7-11’s old numbers are bracketed together in the revision; Ref. 7-10 (Sleeve)’s New No. cell reads “Assy. #” and Ref. 7-11 (Roller) carries the assembly’s own new number.

EXPLODED VIEW 7
PARTS LIST 8
	Ref. No.
	Description
	Parts No.
	New No.

	8-1
	Meter Grille
	AF-207-005
	PZ4A007

	8-2
	Knob B
	NB-31-014
	KN1012

	8-3
	Spacer
	TY-100-038
	PZ1B011

	8-4
	Knob A
	NB-31-013
	KN1011

	8-5
	Spacer
	TY-100-013
	KZ6C015

	8-6
	Variable Resistor Escutcheon
	TY-100-010
	PZ4A006

	8-7
	Push Button B
	NB-19-4094B
	KN2026

	8-8
	Push Button A
	NB-19-4094A
	KN2025

	8-9
	Amplifier Display Panel
	AF-230-003
	A101601

	8-10
	Lamp Cover
	TY-900-024A.B(A:Red,B:Green)
	LU9002

	8-11
	Lamp Assembly
	PL-19-005
	LU2003

	8-12
	VU Meter
	MT-11-023
	ME11003

	8-14
	Blind
	TY-900-029
	PZ1B010

	8-15
	Blind
	TY-900-031
	PZ1B012

	8-16
	Amplifier Mounting Base
	AF-230-004
	A101602

	8-17
	Record out & Playback Equalizer Amplifier Assembly
	PA-286A
	PB-11O

	8-18
	MIC Amplifier Assembly
	PA-287A
	PB-11P

	
	Test Oscillator & Line out Amplifier Assembly
	PA-285
	PB-11N

	8-19
	Variable Resistor
	VR-19-EWF-A0AM25A24
	RV224001

	8-20
	Terminal
	LP-09-STT-1L5NR
	CN901011

	8-21
	Remort Connector [sic]
	CN-09-OSAB12F N/N
	CN212050

	8-22
	Stereo Jack
	CN-09-LJ-109
	CN603009

	8-23
	Slide Switch C
	SW-39-SL242B4
	WH340013

	8-24
	Slide Switch A
	SW-39-SL242B4
	WH340011

	8-25
	Stereo Jack
	CN-09-LJ-110-1-2
	CN602010

	8-26
	Spacer
	TO-230-009
	KZ6C023

	8-27
	Rear Panel
	AF-230-007
	A101609

	8-28
	Rear Hame Plate [sic]
	AF-230-009
	A101610

	8-29
	Connector Supporter
	AF-204-11
	A101610

	8-30
	Connector
	CN-09-XLR-3-31
	CN103046

	8-31
	Connector
	CN-09-XLR-3-32
	CN103045

	8-32
	Fuse Holder
	FS-89-SN-2052
	FH1-022

	8-33
	IC Power Supply
	IC-09-SI-3250E
	ISI3240E

	8-34
	SUB Power Supply PCB Assembly
	PA-307
	PB-61C

	8-35
	Dummy Plug
	CN-01-QS-SP12M N/N
	CN212049

	8-36
	Earth Terminal
	LP-09-T-10
	CN901040

	8-37
	Fuse
	FS-19-2A
	FH7A020

	8-38
	Cord Stopper
	RB-19-BU-3270
	PZ1G002

	8-39
	Power Cord
	TY-559
	PZ9D017


Site note: Ref. No. 8-13 is called out in EXPLODED VIEW 8 but has no corresponding row printed in Parts List 8; the row after 8-18 prints a description and part number with no Ref. No. — both as in the original.
Site note: Ref. 8-10’s row is asterisked in the revision, the same way Ref. 6-27’s is: the New No. cell above (LU9002) is only for the “A:Red” variant. A footnote below the table, keyed by the same asterisk, gives the “B:Green” variant’s new number, transcribed verbatim: “* B:Green … LU9003”

EXPLODED VIEW 8
PARTS LIST 9
	Ref. No.
	Description
	Parts No.
	New No.

	9-1
	Top Packing
	PC-133-002
	K700502

	9-2
	Left Side Packing
	PC-133-007
	K7005-A

	9-3
	MX-5050 Profetional [sic] Assembly
	——-
	

	9-4
	Right Side Packing
	PC-133-008
	K7005-B

	9-5
	Reel Clamper Packing Assembly
	——-
	

	9-6
	Packing B
	PC-133-003
	K700503

	9-7
	Packing C
	PC-133-004
	K700504

	9-8
	Open Reel Box
	———–
	

	9-9
	Packing Box
	PC-133-001
	K700501



EXPLODED VIEW 9
Schematics and Board Layouts
Site note: The remaining pages of the manual are schematic and layout sheets, reproduced here full-size — click any sheet to open it. Note what’s absent: the tape transport wiring diagram is not bound into this manual. The board-layout sheets say so themselves — “Refer to TAPE TRANSPORT ELECTRONICS (TD5050DA) WIRING DIAGRAM” — and that separate fold-out is the tape transport schematic hosted on the manuals page (https://otarimx5050.com/library/manuals/).

SIMPLIFIED DIAGRAM for Models 2S and 4S (at 1kHz)
Site note: The later-revision printing of this sheet adds an “old #” / “new #” header above the title, verbatim: old # (PA-287A), new # PB-11P.

MIC. LINE INPUT & SEL. REP. AMPLIFIER P.C. BOARD ASSY (PA-287A)

MIC,LINE INPUT & SEL.REP AMPLIFIER P.C.BOARD ASSY PA287A(PM918A)

REC OUTPUT & REP.EQUALIZER AMPLIFIER P.C.BOARD ASSY PA286A(PM917A)
Site note: The later-revision printing of this sheet adds an “old#” / “new #” header above the title, verbatim: old# (PA-286A), new # PB-11O.

REC. OUTPUT & REP. EQUALIZER AMPLIFIER P.C. BOARD ASSY (PA-286A)
Site note: The later-revision printing of this sheet adds an “old #” / “new #” header above the title, verbatim: old # (PA-285), new # PB-11N.

TEST OSC. & LINE OUTPUT AMPLIFIER P.C. BOARD ASSY (PA-285)

TEST OSC & LINE OUTPUT AMPLIFIER P.C.BOARD ASSY PA285(PM680-1)
Site note: The later-revision printing of this sheet adds an “old #” / “new #” header above the title, verbatim: old # PA-377 (PM-875A), new # PB-61E.
 [sic]
Site note: The later-revision printing of this sheet adds an “old#” / “new #” header above the title, verbatim: old# PA426(PM796), new # PB-61D.

+5 VOLT DC POWER SUPPLY P.C.BOARD ASSY PA426(PM796)
Site note: The later-revision printing of this sheet adds an “old #” / “new #” header above the title, verbatim: old # PA284(PM679-2), new # PB-41D.

CONTROL P.C.BOARD ASSY PA284(PM679-2)
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  BRACKET MOUNTING SCREWS (4) CAPSTAN MOTOR PRINTED CIRCUIT BOARD DRIVE BELT
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  MOUNTING PLATE B;FOUR M3 CROSS HEAD SCREWS SERVO CONTROL P.C.B. Ass’y CONNECTOR POWER SUPPLY P.C.B. Ass’y A;FOUR M4 CROSS HEAD SCREWS C;THREE M4 CROSS HEAD SCREWS
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  RING A RING B BRAKE SOLENOID BRAKE SPRING BRAKE LEVER SOLENOID PIN STROKE 0.2±0.02inch (5±0.5mm) TWO CROSS HEAD SCREW TOW HEXAGONAL SOCKET SCREW BRAKE DRUM BRAKE BAND BRAKE GUIDE CORD CRAMPER (BRAKE BAND GUIDE)
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  PINCH ROLLER CAP WASHER PINCH ROLLER
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  HEAD BASE 1/4” FOR FULL OR 2 TRACK 7/32” FOR 4 TRACK BRAKET SPACER ¾”, APPROX TAPE ERASE HEAD REPRODUCE HEAD 4T RECORD HEAD REPRODUCE HEAD 2T
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  SPACERS 1/4” DIA x 3/4” TAPE
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  PARALLEL POSITION ZENITH EQUAL ANGLE TAPE WRAP RIGHT ANGLE AZIMUTH


rId132.svg
  
 
Created by potrace 1.16, written by Peter Selinger 2001-2019

 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 

  STANDARD UNBALANCE INPUT 3 2 1 47K 10K 82K OPTIONAL BALANCED INPUT 3 2 1 220Ω 220Ω 220Ω 220Ω 220Ω 1 5 4 8 82K 600Ω ET-21-181
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  1 5 3 6 4 2 A Take out jumpers 1 and 2. B UM-solder 3 and solder to 5. C UM-solder 4 and solder to 6.
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  TO P.C. B LINE INPUT 1 2 3 WHITE ORANGE SHIELD
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  OUTPUT LEVEL SW 3K 600Ω 3 2 1 STANDARD UNBALANCED OUTPUT OUTPUT LEVEL SW 3K 1 5 2 8 OUTPUT 600Ω 3 2 1 SHIELD ET-31-182 OPTIONAL BALANCED OUTPUT
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  600Ω¼W 2 1 3 1 5 2 6 3 7 4 8 WHITE ORANGE SHELD
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  EXPLODED   VIEW   1 1-11 1-10 1-3 1-11 1-4 1-10 1-1 1-9 1-8 1-9 1-9 1-9 1-9 1-8 1-9 1-5 1-1 1-7 1-7 1-7 1-6


rId164.svg
  
 
Created by potrace 1.16, written by Peter Selinger 2001-2019

 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 

  EXPLODED   VIEW   2 2-1 2-2 2-1 2-3 2-2 2-4 2-1 2-4 2-2 2-1 2-2 2-5 2-1 2-1 2-2 2-1 2-2 2-1 2-2 2-2 2-6 2-7 2-8 2-9 2-11 2-10 2-9 2-11 2-12 2-13 2-14 2-15 2-16 2-17
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  EXPLODED   VIEW   3 3-1 3-2 3-3 3-4 3-5 3-6 3-7 3-8 3-16 3-11 3-9 3-12 3-17 3-13 3-10 3-14 3-15 3-15 3-18 3-19 3-20 3-21 3-22 3-23 3-32 3-24 3-25 3-33 3-25 3-26 3-26 3-32 3-28 3-27 3-29 3-28 3-33 3-30 3-29 3-34 3-35 3-34 3-35 3-30 3-31 3-32 3-31 3-32 3-27


rId172.svg
  
 
Created by potrace 1.16, written by Peter Selinger 2001-2019

 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 

  EXPLODED   VIEW   4-1 (For   Models   2S   and   4S) 4-1 4-2 4-3 4-4 4-5 4-6 4-7 4-8 4-9 4-9 4-10 4-11 4-12 4-13 4-13 4-14 4-15 4-16 4-17 4-18
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  EXPLODED   VIEW   4-2 (For   Models   2SD   and   4SD) 4-101 4-103 4-104 4-106 4-105 4-108 4-106 4-109 4-110 4-111 4-112 4-113 4-111 4-114 4-115 4-116 4-102 4-107
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  EXPLODED   VIEW   5 5-1 5-2 5-3 5-2 5-6 5-4 5-7 5-5 5-8 5-9 5-24 5-10 5-22 5-22 5-10 5-11 5-23 5-25 5-13 5-26 5-27 5-14 5-12 5-28 5-15 5-27 5-16 5-17 5-20 5-32 5-4 5-18 5-33 5-19 5-34 5-21 5-35 5-4 5-29 5-30 5-31 5-12
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  EXPLODED VIEW 6 6-4 6-1 6-2 6-3 6-7 6-5 6-6 6-8 6-9 6-10 6-11 6-12 6-14 6-15 6-13 6-16 6-19 6-21 6-17 6-18 6-20 6-22 6-23 6-24 6-25 6-26 6-27 6-28 6-29 6-30 6-31 6-32 6-37 6-38 6-33 6-34 6-39 6-35 6-36 6-40 6-40 6-41 6-41 6-42 A B
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  EXPLODED   VIEW   7 7-1 7-2 7-1 7-3 7-2 7-4 7-3 7-5 7-4 7-6 7-5 7-7 7-6 7-8 7-9 7-10 7-11 7-8 7-12 7-13 7-14 7-15 7-16 7-17 7-17 7-18 7-18 7-19 7-19 7-23 7-20 7-24 7-21 7-25 7-22
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  EXPLODED   VIEW   8 8-2 8-3 8-4 8-2 8-1 8-4 8-3 8-4 8-5 8-6 8-7 8-5 8-8 8-9 8-10 8-10 8-10 8-14 8-11 8-12 8-13 8-14 8-14 8-15 8-17 8-18 8-16 8-23 8-22 8-25 8-18 8-19 8-20 8-21 8-34 8-24 8-38 8-26 8-27 8-39 8-28 8-29 8-38 8-31 8-33 8-30 8-35 8-36 8-37 8-32 8-7 8-5 A A B B A
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  EXPLODED   VIEW   9 9-1 9-2 9-3 9-4 9-5 9-6 9-7 9-8 9-9
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  DEMAGNETIZER


rId200.svg
  
 
Created by potrace 1.16, written by Peter Selinger 2001-2019

 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 

  SIMPLIFIED DIAGRAM for Models 2S and 4S (at 1kHz) Values in the parentheses is on models 4S(D) MIC AMPL. 34 MIC INPUT -70dBm LINE INPUT -5dBm 47K NOR 10K OSC -36dBm -47dBm MIC INPUT LINE INPUT AMPL. 40 -21dBm LINE INPUT REC LEVEL CAL. -6dBm (-7dBm) -12.5dBm (-13.5dBm) REC. EQ REC. OUTPUT AMPL. BIAS OSCILLATOR 133kHz BIAS CURRENT ADJ. ERASE HEAD CHECK POINT 10Ω ERASE CURRENT 80 mA (45 mA) REC. HEAD CHECK POINT REC. NOR. 100Ω BIAS CURRENT 2.5 mA (2.0 mA) SIGNAL CURRENT 175μA(155μA) ( SCOTCH 206 PEAK BIAS ) TEST OSC. SEL. REP. AMPL. 29 -36dBm (-41dBm) -65dBm (-70dBm) SEL. REP. LEVEL SEL. REP. NOR. REP. HEAD -50dBm (-55dBm) REP. EQ REP. EQ AMPL. 35 -15dBm (-20dBm) MRL. ADJ. SRL. CAL. SOURCE TAPE -30 dBm NOR SRL OUTPUT LEVEL LINE OUTPUT AMPL. +4dBm 3K HI LO 600Ω LINE OUTPUT +4dBm:HIGH -10dBm:LOW HEAD PHONE AMPL HEAD PHONE -24dBm METER AMPL. METER CAL. VU METER
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  MIC,LINE  INPUT  &  SEL.REP  AMPLIFIER  P.C.BOARD  ASSY  PA287A(PM918A) R372 C375 R374 R382 C373 R373 TR371 C374 R378 R380 TR372 R379 R383 R381 C380 C379 C378 R376 C383 C384 R384 R385 C385 R386 SW4 +B +24V C371 C351 C372 C376 C362 C356 R375 R355 C363 TR351 C354 R377 R357 R356 R351 C360 C359 C358 R352 R354 C355 R360 R358 TR352 R359 R363 R364 R5 R4 C2 R8 C6 R6 TR101 TR102 R1 R3 R1 R3 C3 C3 C27 C27 R7 R7 C8 R17 R19 R22 R18 R22 R18 C7 C11 R24 C14 C14 TR104 R130 R26 SW2 C17 TR3 R24 R21 R20 C13 C15 R23 R25 C16 C17 TR1 TR2 C2 R6 R4 R5 C4 C6 R8 R16 R17 C7 C9 R371 C377 C367 C381 C361 C382 C362 R367 R328 R325 SW1 C16 R362 R30 TR103 R387 R365 C363 R10 R11 C10 R2 C1 R11 R10 R16 C10 C9 R20 R21 C13 C1 R2 R353 C4 C15 R25 R23 R26 C8 C11 C364
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  REC OUTPUT & REP.EQUALIZER AMPLIFIER P.C.BOARD ASSY PA286A(PM917A) R165 R65 R128 R28 R129 R29 R138 R38 R164 R141 R41 R322 C58 C119 C118 C19 C18 C122 C121 C120 C22 C21 C20 C23 C23 C301 R301 D151 D51 TR115 TR15 R61 R61 LEVEL R163 R57 R57 C57 EQ TR108 TR8 R97 R97 R58 R58 R59 C56 R59 R56 C54 C54 TR107 TR7 R56 R55 R55 R54 R54 R53 TR106 TR6 C73 C73 R96 R92 C52 C52 C51 C51 R51 R51 R30 R30 R32 R27 R32 R27 R33 R31 R33 R31 TR105 TR5 L101 L1 C26 C25 C25 C26 R35 R34 R34 R35 R38 R38 L102 L2 C55 C57 C24 C24 C29 C30 C27 C28 C29 C30 C27 C28 RL3 R37 R37 D301 C31 C31 REC. AMPL. +B R302 L301 C303 C302 R304 R303 D303 D302 C132 C32 C307 TR302 TR301 R306 R305 R307 R309 R308 R311 R315 R316 R310 TR303 R312 TR304 TR305 TR306 R313 R314 TR307 TR308 R318 R317 R319 R320 R321 C304 C305 C306 C55 R98 R160 R62 R62 R60 R96 R92 R63 R36 R36
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  TEST OSC & LINE OUTPUT AMPLIFIER P.C.BOARD ASSY PA285(PM680-1) C159 C160 R168 TR109 R170 C161 R167 R166 C162 R171 C165 R174 C163 TR110 R183 TR112 R182 TR111 R177 R178 C171 OUT-2 OUT-1 E R186 R173 L151 R172 R181 R176 R184 R190 R189 C166 2·VU C170 R187 R188 C169 R192 R193 TR114 R195 R194 C172 R191 C168 ET11-096 H PHONE·2 R175 R180 L51 C62 R179 SV·2 R81 C65 R80 C167 C164 E TR12 R83 R82 TR11 SV·2 R92 R77 TR9 E C64 TR10 E R79 R72 C63 R76 R73 C61 R67 R69 R70 C60 R68 C59 SW6·1 R80 C67 C68 R91 R89 R87 TR13 R90 R88 C71 C70 1·VU C69 R94 R95 R93 C72 C66 R207 C203 C205 R210 TR202 R202 R209 R204 R208 C204 R206 E C201 C202 R203 R205 TR201 E H PHONE·1 ET11-096 C207 CH1·IN CH2·IN R13 VR·2 R114 R211 R117 R12 R201 LIN VR
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  CAPSTAN SERVO MOTER POWER SUPPLY P.C. BOARD ASSY PA-377 (PM-875A) Refer to TAPE TRANSPORT ELECTRONICS(TD5050DA) WIRING DIAGRAM 1 2 3 4 5 6 7 8 9 10 11 12 14 15 16 17 18 19 20 21 A B C H L 1 2 E B C RL1 RL2 R13 D8 D7 Q2 E R9 C5 E Q3 R10 C6 R7 R8 C4 C2 C1 R6 R5 R3 R4 R2 R1 C7 E Q1 IC1 D5 D6 D2 D3 D1 D4
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  +5 VOLT DC POWER SUPPLY P.C.BOARD ASSY PA426(PM796) Refer to TAPE TRANSPORT ELECTRONICS(TD5050DA) WIRING DIAGRAM 2 3 4 5 IN EMITTER BASE GND OUT COLLECTOR R2 R1 Q1 C1 C2 IC1 B E PM796 1 3 2
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  CONTROL P.C.BOARD ASSY PA284(PM679-2) Refer to TAPE TRANSPORT ELECTRONICS WIRING DIAGRAM R21 TR4 E R16 R15 C14 C R11 R13 R14 D11 11 D6 D7 11 20 R22 D18 21 22 23 105 104 106 103 107 R46 C19 102 34 RL-A b2 RL-A b1 1 2 C8 SCR1 R10 C13 13 12 TR1 E C45 C9 D12 10 TR3 D8 D9 SCR2 C 25 R26 C42 R47 100 R48 TR12 R49 C43 D3 D5 D4 C6 SCR3 TR6 E C C20 R29 R30 TR13 E D19 TR14 E C4 RL-B RL-B 4 5 6 TR2 E C10 R5 D15 R39 C24 E RL-C C11 R33 R36 R31 TR9 C22 29 C3 31 RL-C C2 R17 D17 C15 E TR5 C21 D20 E R45 3 C38 C37 L35 C16
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  PINCH ROLLER CAP PINCH ROLLER DUST CAP FELT COLLAR
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  SUPPLY TAKE UP A B B A
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  BRAKE SPRING BRAKE LEVER BRAKE SOLENOID STROKE 0.2±0.02inc (5±0.5mm) BRAKE DRUM BRAKE BAND BRAKE GUIDE CORD CRAMPER (BRAKE BAND GUIDE)
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  SLINDER “C” SLINDER “B” SLINDER “A” FRONT PANEL
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  CAPSTAN SOLENOID PINCH ROLLER PRESSURE NUT LOCK NUT
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  L M H CAPSTAN SERVO CONTROL P.C. BOARD


rId60.svg
  
 
Created by potrace 1.16, written by Peter Selinger 2001-2019

 
 
 
 
 
 
 
 

  C1 0.047µF, 5% (MYLAR) R1 12K, 5% ¼W RECORDER LINE OUT R2 110K ¼W, 5% 650PF 5% (MICA) TO VTVM POMONA ELECTRONICS MODEL MDP-X OR EUIV DRILL & TERMINAL LUG MOUNT (OPTIONAL) POMONA ELECTRONICS MODEL MDP-X OR EUIV C1 R2 C2 R1 GND
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  BRANK TAPE TEST TAPE
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  BIAS CAL REC EQ HIGH SPEED LOW SPEED SRL CAL CH 1 CH 2 CH 1 CH 2 CH 1 CH 2 CH 1 CH 2 R38 R138 R29 R129 R28 R128 R65 R165 MAX REP LEVEL CH1 R63 CH2 R163 REP EQ CH1 R60 CH2 R160 REPRODUCE EQUALIZER AMPL. BIAS OSCILLATOR RECORD OUTPUT AMPL PA286A REC OUTPUT & REP EQUALIZER AMPL. ASSY REC CAL (SOURCE LEVEL) CH1 R30 CH2 R130 SEL REP LEVEL CH1 R367 CH2 R387 LINE INPUT AMPL SELECTIVE REPRODUCE AMPL MICROPHONE INPUT AMPL. PA287A MIC. LINE INPUT & SEL REP AMPL. ASSY TEST OSCILLATOR R80 BIAS TRAP L51 CH1 LINE OUTPUT AMPL. R74 R180 R174 R86 CH1 VU METER CAL R186 CH2 BIAS TRAP L151 CH2 PA285 TEST OSC. & LINE OUTPUT AMPL. ASSY ADJUSTMENT REQUIRED NO ADJUSTMENT REQUIRED (FACTORY ADJUSTS)
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  THREE REEL TABLE FIXING SCREWS TWO REEL TABLE HEIGHT SCREWS FOUR MOTOR MOUNTING NUTS FOUR MOTOR MOUNTING CROSS HEAD SCREWS


